

EC Declaration of product conformity

PPE regulation(2016/425)



The following model of Personal Protective Equipment has been subjected to EU-type examination in accordance with the module B of the PPE regulation (2016/425) and has been shown to satisfy to essential health and safety requirements.

NANTONG JIADELI SAFETY PRODUCTS CO.,LTD Tel: +86 21 61372112

Shuangdian Industrial Park C,Rudong county, Fax:+86 21 61372113

Jiangsu Province,China www.jdlsafety.com

Declares that the product described hereafter:

Glove description:13 gauge Steel Core yarn, ANSI cut Level A8/ ISO 13997 Cut Level F shell

Foam nitrile coating on palm

Style no:ND6574 Medium risk, category II



**4X43F**

Is in conformity with the provisions of the PPE regulation(2016/425) and with the European harmonised standards EN 420:2003+ A 1:2009, EN 388:2016 and is identical to the PPE which is subject to EC Type Examination Certificate 0075/1203/162/06/12/0415EXT 01/08/12, 02.08.2012, issued by Notified Body 0075

CTC

4, rue Hermann Frenkel

69367 Lyon Cedex 07

France

Shanghai 17.09.2018